Note to Specifier: Delete/Update as necessary

* **Description:** Security Roller Shutter System
* **Product reference:** **Xonar 964 Roller Shutter**
* **Manufacturer:** CGT Security
* 1 Darwin Close, Reading, Berkshire, RG2 0TB
* Tel: 0330 024 9409
* Email: [sales@cgtsecurity.com](mailto:sales@cgtsecurity.com)
* **Standards:** ISO 9001
* **Product Certification/Performance**: Product certified to LPS 1175 Issue 7, security rating 4 (SR4), Secured By Design Official Police Preferred Specification.
* **Arrangement:** Horizontal shutters, with roller shutter boxes mounted at high level.
* **Opening Sizes:**
  + External face fit
    - Maximum certified width 6000mm
    - Minimum certified width 1000mm
    - Maximum certified height 10000mm
    - Minimum certified height 1800mm
  + Internal face fit
    - Maximum certified width 6000mm
    - Minimum certified width 1000mm
    - Maximum certified height 10000mm
    - Minimum certified height 1000mm
* **Shutter Curtain:**
  + **Material:**  Extruded aluminium lath profile to grade 6063 T6 with reinforced cores.
  + **Finish:** Polyester powder coated to 25 microns.
  + **Colour:**  Standard RAL/BS code
* **Frame/Guides:**
  + **Material**: Heavy duty extruded aluminium guide profiles to grade 6063 T6, anchored direct to the structure.
  + **Finish:** Polyester powder coated to 25 microns.
  + **Colour:** Standard RAL/BS code
* **Bottom Rail:**
  + **Material**: Reinforced extruded aluminium section with strengthened core.
  + **Finish:** Polyester powder coated to 25 microns.
  + **Colour:** Standard RAL/BS code
* **Operation:** Self-locking technology. Motorised to allow controlled ascent and descent. Shutter to automatically lock into position upon descent without manual intervention or key locking.
* **Motor**
  + Tube Motor - Low duty cycle, or where limited to single phase supply
  + External Drive Motor - High duty cycle or for larger apertures
  + Smooth and quiet operation with roller guide entry
* **Suitable Substrate:** to be mechanically anchored directly to blockwork, concrete, structural steelwork, or sub assembly steel framework as certified to LPS 1175 issue 7, security rating 4 (SR4).
* **Operation/Controls:** Full range of compatible controls including
  + Push button switch/key switch/Radio control/or possible to integrate into building management systems and third party alarms
  + Safety on close as assessment directs
  + High duty cycle motor and battery backup options
* **Installation & Fixing:** In accordance with CGT Security Installation guidelines and recommendations.

Specification applies to the standard product. Our range of options usually allows us to accommodate any differences you may require. Certain options may affect performance levels. Please contact us and we will be happy to support in developing this specification to meet your exact project requirements.